# Specification

|  |  |  |
| --- | --- | --- |
| **Element** | **Quantity** | **Notes** |
| Three phase source | 2 | * 11 kV, 50 Hz * No internal impedance |
| Bus | 6 | * With voltage measurement |
| LV Load | 2 | * Connected downstream of transformers * Set to any reasonable value |
| HV Load | 2 | * Connected upstream of transformers * Set to any reasonable value |
| Transformer | 2 | * Ratio 11 kV: 0.4 kV * Set rating and impedances to any reasonable value * With power measurement |
| RL line | As necessary | * With current measurement * Set impedance to any reasonable value |
| Switch | 1 | * Changes LV network topology configuration |

